붙임1		KoVAC 공동제작센터 인프라지원 시설 및 장비 안내

□ 시설 개요

○ 상암동 한국VR‧AR콤플렉스(KoVAC) 공동제작지원센터* 內 고품질 LED 기반 XR Stage(VP 제작 스튜디오) 및 K-실감스튜디오(모션캡쳐) 시스템

* 총 2,300여 평 규모로 공동제작센터 1층 특수 촬영 스튜디오(약 450평) 내 XR Stage 및 Chroma Board 구성

① (K-실감스튜디오) 메타버스 및 XR 등의 가상 융합 기반의 입체 디지털휴먼 제작 지원을 위한 광학식 모션캡쳐* 공동 활용 지원 시설

* 사람의 움직임을 360°에서 광학 촬영하여 동작 데이터를 생성하고 3D 툴에서 제작된 모델에 적용하여 입체 디지털 휴먼 시각화를 위한 데이터 생성 기술

② (XR Stage) 시 공간에 구애받지 않고 표현 방식 자율성을 갖춘 차세대 가상 융합 기반 LED Virtual Production 제작 솔루션

* XR Stage : XR Stage 전용 LED 시스템을 통해 실사와 컴퓨터그래픽 혹은 실사기반으로 제작된 가상공간의 합성을 통한 콘텐츠 제작 시스템

□ NIPA XR Stage 시스템 구성

LED Stage	Crane	Tracker

○ XR Stage

- 28m×6m(LED Wall), 6m×12m(Ceiling) 16m×6.5m(Bottom), 2.3m×3.5m(Side Effect) 커브 구조 LED Stage
(Pixel Pitch 2.8mm(Wall), 4.6mm(Bottom), 5.0mm(Ceiling, Side Effect))

- LED Processor : Brompton

- Media Server(Disguise VX4+ 2set, RX 3set, Pixera, ICVFX Ndisplay Server 4set),
센서방식 Tracker 2set(Stype or Mo-sys) * Disguise Latest version

- LED Spot Light(ARRI Obiter 5set & 1KW 3set, 2KW 2set) 및 DMX Controller

○ Chroma Board

- LED XR Stage 연계 15m x 10m x 5m Chroma Wall

- Chroma VP Engine(Zero Density*) 4set, IR Tracker 4set(NCam)

* Unreal Engine Version 4.9

○ 촬영 장비

- Camera : 4K EFP Camera (HDC4300, CCU, RCP 포함)
4K ENG Camera(Venice, 12G Quad)

- Crane 1set Height-25ft (7.6m), Reach-18ft (5.4m)

- 4K Switcher, File Recorder(Shogun, KiPro), Floor Monitor 등

□ NIPA K-실감스튜디오 시스템 구성

Capture Stage		Accessory

○ Motion Capture System

- Stage Size : 12m(가로)×12m(세로)×5m(높이)

- Motion Capture Camera : Optitrack Prime X41(34ea), X13(16ea)

- Motion Capture System : Optitrack Motive 3.0

- Accessory

․Full Body Suit(5ea, S/M/L/XL), Head Rig(5ea), 일체형 Head Rig(Yanus 2ea)
Capture Globe(Manus 8ea, Rococo 5ea), Foot Wrap(5ea)

- Capture용 PC는 별도로 설치 가능하나 원상복구 필수